IF YES

**START**

**CLOSE SOCKET**

Display CRC Value by doing repeated XOR

Display T(x) with zeroes

Display T(x)(Dividend) and g(x)(Divisor)

Connection Established

IF NO

Listen State?

Creation of Socket

Port Number

IP Specification

Socket Variables