**Client Side**

No

Error

occur

If error

YES

NO

Send ACK

Stop

Retransmit

Close socket

Send NACK

Display quotient, reminder CRC

Read T(x), g(x)

Call Connect

Declare variables for socket

Start

Creation of socket

Specify IP Port No.